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DARRIAN T90
FRONT CHASSIS CONVERSION TO DOUBLE WISHBONE 2013
This spec is for owners that wish to update an existing swing axle type car to double wishbone.

OUTLINE OF CHASSIS WORK
Remove front ¼ covers behind front wheels and dig out foam.

Cut away front chassis section/inner arches to front of flat floor.

Prep. front bulkhead/foot wells 

Fit and bond in new double wishbone front chassis section 

Fit and bond in new front covers and foam fill.

Fit and bond in new type front bulkhead/cover.

Drill suspension bracket mounting holes.

£

Labour………..                       





1,500.00 




New type front chassis section 
 
   


  
   750.00

1 pr front cover panels   


                                               
     30.00

I front bulkhead/cover



                                 
   100.00                 







Total front chassis              2,380.00 

SUSPENSION 
Front suspension mount plate and all top & bottom pivot brackets

   200.00

Front double wishbone kit inc. joints, rod ends, bushes etc.


   800.00

Front billet uprights inc. steering arms and spacers etc.


   860.00

Sierra front axles and housings (Exchange) 




   100.00 pr.

Front wheel bearings






     50.00 set

High ratio Titan steering rack – to spec




   350.00

Comp. track rods complete





   120.00

Billet rack mounts 





                  100.00    






Total suspension

2,580.00
Total less VAT

4,960.00




VAT @ 20%

   992.00






TOTAL

             £5,952.00
Group A or Group 4 wheel studs are extra










For further suspension items, dampers, rear arms etc. please see suspension spares list or main brochure.

TERMS:     
50% on commencement of order,

 Balance payable on collection
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